# TOP VIEW

Ø32" TWIST & LOCK LID W/

INFLATABLE WATERTIGHT SEAL

LOCKING TABS FOR PADLOCK

2'-8 1/4" I.D.

1'-6"

TOP 18" GEL-COAT

# ISOMETRIC VIEW

A

2'-6" I.D.

Ø30" FRP RISER W/ BELL END FOR EPOXY SOCKET

3"

SHEET TITLE:

Ø30" FRP RISER W/ Ø32" TWIST & LOCK WATERTIGHT LID

DRAWN DATE:

08/14/21

DRAWN BY:

JACK

REV.

00

2'-7"

2'-7 1/2"

# FRONT VIEW

Mailing: P.O. BOX 326, Montreal, MO 65591 MFG: 147 Opportunity Rd.,

Camdenton, MO 65020

P: 573-317-9620