FLAT BAFFLE WALLS

FLOW THROUGH HOLES

CROSSOVER INVERT IF APPLICABLE

A

FULL FLAT BAFFLE

FLOW THROUGH HOLES

CROSSOVER INVERT IF APPLICABLE

A

A

7/8 FLAT BAFFLE

BAFFLE CROSSOVER WILL BE: (PLEASE CHECK ONE)

IF USING FLOW-THROUGH HOLES:

A

FLOW THROUGH HOLES CROSSOVER PIPING

DIAMETER OF HOLE (S) QUANTITY OF HOLE (S)

SHEET TITLE:

SELECTION GUIDE

PROJECT:

FLAT BAFFLE WALLS



1/2 FLAT BAFFLE

BAFFLE MUST PROVIDE A SOLID BARRIER FOR LIQUIDS/ SOLIDS SEPARATION

YES NO

DRAWN DATE: DRAWN BY: REV.

01/10/20 JACK 00

P.O. BOX 326, Montreal, MO 65591 P: 573-317-9620