|  |
| --- |
| **FRP FULL COUPLING****PVC PIPE STUB****FRP FLANGE NOZZLE WITH CONE GUSSET** |
| STANDARD PIPE STUB AND COUPLING O.D.SIZES |  |
|  | STANDARD FRP NOZZLE SIZES | FRP FLANGED NOZZLE NOTES:- ALL BOLTING PATTERNS CONFORM TO ANSI B16.5 150# STANDARD. |
| DIA. | SCH80 PIPE STUB O.D. | SDR-35 PIPE STUB O.D. | FRP PIPE STUB O.D. | FRP COUPLING I.D. | NOZZLE DIA. | # OF BOLTS | CIRCLE DIA. | HOLE DIA. | FLANGE DIA. | PROJECT HGT. |
| 2" | 2.375" | N/A | 2.5" | 2" | 2" | 4 | 4 3/4" | 3/4" | 6" | 6" | WITH CONE GUSSETS |  |
|  | SHEET TITLE:LOCATIONS |
| 3" | 3.5" | N/A | 3.5" | N/A | 4" | 8 | 7 1/2" | 3/4" | 9" | 6" |
| PROJECT:FULL FRP COUPLING PVC PIPE STUBFRP FLANGE NOZZLE |
| 4" | 4.500" | 4.215" | 4.5" | 4" | 6" | 8 | 9 1/2" | 7/8" | 11" | 6" |  |
| 6" | 6.625" | 6.275" | 6.5" | 6" | 8" | 8 | 11 3/4" | 7/8" | 13 1/2" | 6" |
| DRAWN DATE:01/07/20 | DRAWN BY:JACK | REV.00 |
| 8" | 8.625" | 8.400" | 8.5" | 8" | 10" | 12 | 14 1/4" | 1" | 16" | 6" |
| P.O. BOX 326, Montreal, MO 65591 P: 573-317-9620 |
| 10" | 10.750" | 10.500" | 10.5" | N/A | 12" | 12 | 17" | 1" | 19" | 6" |
| 12" | 1'-0.75000" | 12.500" | 12.5" | N/A | 14" | 12 | 18 3/4" | 1 1/8" | 21" | 6" |

