# STRAIGHT PIPE SINGLE 90°

# DOUBLE 90°

NOTE:

* SITE SPECIFIC DATA ( ) MUST BE FILLED IN BY SPECIFIER, OWNER OR INSTALLING CONTRACTOR.

-ALL CROSSOVER PIPING IS SCHEDULE 40 PVC.

* THIS FORM MUST BE ACCOMPANIED BY THE BAFFLE / PARTITION WALL DRAWING.

8"

PIPE DIA.

PIPE DIA.

PIPE DIA.

# SINGLE TEE

A

**DOUBLE TEE**

VENT PIPE LENGTH

A

DOWN PIPE LENGTH

A

VENT PIPE LENGTH

DOWN PIPE LENGTH

VENT PIPE LENGTH

DOWN PIPE LENGTH

A

A

SHEET TITLE:

A

SELECTION GUIDE

PROJECT:

BAFFLE/ PARTITION CROSSOVER PIPE AND TEE

PIPE DIA.

PIPE DIA.

DRAWN DATE:

01/08/20

DRAWN BY:

JACK

REV.

00



P.O. BOX 326, Montreal, MO 65591 P: 573-317-9620