1 1/2"

15/16"

## 3/4"-10 UNC, CLASS 2A

5/8"

## 26" CLOSED EXPANDING TO 44"

28 1/2"

# 3/4" X 18" JAW TO JAW TURNBUCKLE

5/8"

15/16"

1 1/2"

## 3/4"-10 UNC, CLASS 2A

## 20" CLOSED EXPANDING TO 32"

22 1/2"

# 3/4" X 12" JAW TO JAW TURNBUCKLE

5/8"

3/4"

1 1/4"

15/16"

1 1/2"

## 3/4"-10 UNC, CLASS 2A

## 17" CLOSED EXPANDING TO 26"

1'-7 1/2"

3/4"

5 1/2"

# 3/4" X 9" JAW TO JAW TURNBUCKLE

1 1/4"

PROJECT NAME:

JAW TO JAW TURNBUCKLES

|  |
| --- |
| TURNBUCKLE SELECTION GUIDE |
| TANK SIZE & APPLICATION | TURNBUCKLE SIZE |
| Ø4' TANK W/ CONCRETE DEADMEN ABOVE BEDDING | N/A |
| Ø4' TANK W/ CONCRETE DEADMEN BELOW BEDDING | 3/4" X 9" |
| Ø4' TANK W/ FRP DEADMEN | 3/4" X 6" |
| Ø5' TANK W/ CONCRETE DEADMEN ABOVE BEDDING | N/A |
| Ø5' TANK W/ CONCRETE DEADMEN BELOW BEDDING | 3/4" X 9" |
| Ø5' TANK W/ FRP DEADMEN | 3/4" X 6" |
| Ø6' TANK W/ CONCRETE DEADMEN ABOVE BEDDING | N/A |
| Ø6' TANK W/ CONCRETE DEADMEN BELOW BEDDING | 3/4" X 9" |
| Ø6' TANK W/ FRP DEADMEN | 3/4" X 6" |
| Ø8' TANK W/ CONCRETE DEADMEN ABOVE BEDDING | 3/4" X 12" |
| Ø8' TANK W/ CONCRETE DEADMEN BELOW BEDDING | 3/4" X 12" & 3/4" CONN. LINK |
| Ø8' TANK W/ FRP DEADMEN | 3/4" X 12" |
| Ø10' TANK W/ CONCRETE DEADMEN ABOVE BEDDING | 3/4" X 18" |
| Ø10' TANK W/ CONCRETE DEADMEN BELOW BEDDING | 3/4" X 18" |
| Ø10' TANK W/ FRP DEADMEN | 3/4" X 18" |
| Ø12' TANK W/ CONCRETE DEADMEN ABOVE BEDDING | 3/4" X 18" |
| Ø12' TANK W/ CONCRETE DEADMEN BELOW BEDDING | 3/4" X 18" |
| Ø12' TANK W/ FRP DEADMEN | 3/4" X 18" |

# 3/4" CONNECTING LINK

15/16"

5/8"

1 1/2"

## 3/4"-10 UNC, CLASS 2A

DRAWN DATE: DRAWN BY: REV.

## 08/31/21 JACK 01

## 14" CLOSED EXPANDING TO 21"

16 1/2"

# 3/4" X 6" JAW TO JAW TURNBUCKLE

Mailing: P.O. BOX 326, Montreal, MO 65591 MFG: 147 Camdenton Bus. Prk. Dr., Camdenton, MO 65020

P: 573-317-9620