F E F

C

K

B O

G L

M

D A P P N

I

J

H

INDUSTRIAL WASTEWATER/ CHEMICAL WASH DOWN TANK (DOUBLE WALL TANK)


[www.fgtsolutions.com](http://www.fgtsolutions.com/) Phone: 573-317-9620

|  |  |  |  |
| --- | --- | --- | --- |
| BILL OF MATERIALS | | | |
| ITEM | DESCRIPTION | ITEM | DESCRIPTION |
| A | Ø24" MANWAY W/ STEEL COVER | I | LEVEL SENSORS |
| B | Ø42" CONTAINMENT COLLAR W/ EPOXY SOCKET | J | 4" FLANGE NOZZLE W/ FIBERGLASS DROP PIPE |
| C | Ø42" CONT. SUMP W/ Ø37" WATERTIGHT TWIST LOCK LID | K | 4" PUMP OUT CONNECTION W/ CAM-LOCK QUICK CONNECT |
| D | 4" HALF COUPLING, NPT MANWAY COVER FITTING | L | 6" FLANGE NOZZLE INLET |
| E | Ø42" H-20 RATED STEEL MANHOLE RING & COVER | M | 6" FLANGE X FLANGE FLEXIBLE CONNECTOR |
| F | Ø16" H-20 RATED STEEL MANHOLE RING & COVER | N | 4" HALF COUPLING, NPT |
| G | 4" HALF COUPLING, NPT INTERSTITIAL MONITOR FITTING | O | 4" VENT LINE |
| H | LEAK DETECTION SENSOR | P | STEEL LIFTING LUGS |

MFG: 147 Opportunity Rd., Camdenton, MO 65020

DATE:

8/18/2021

Mailing: P.O. BOX 326, Montreal, MO 65591