# ISOMETRIC VIEW

**TOP VIEW**

STEEL OR FRP COVER 1/8" THICK GASKET

MANWAY DIMENSIONS

SIZE **22" 24" 30"**

O.D. 28" 32" 38 3/4"

I.D. 22" 24" 30"

BOLT CIRCLE

6"

HOLE Ø

26"

3/4"

29 1/2"

1/2"

36"

3/4"

SHEET TITLE:

FIBERGLASS MANWAYS

HOLE QTY 24

20 28

DRAWN DATE:

11/12/20

DRAWN BY:

JACK

REV.

00

# FRONT VIEW

12"

Mailing: P.O. BOX 326, Montreal, MO 65591 MFG: 147 Camdenton Bus. Prk. Dr., Camdenton, MO 65020

P: 573-317-9620