G F G

Q Q C N L

B

H O

M

P D E P D A

J

K

I

MEDICAL DECONTAMINATION TANK (DOUBLE WALL TANK)

BILL OF MATERIALS


[www.fgtsolutions.com](http://www.fgtsolutions.com/) Phone: 573-317-9620

|  |  |  |  |
| --- | --- | --- | --- |
| ITEM | DESCRIPTION | ITEM | DESCRIPTION |
| A | Ø24" MANWAY W/ STEEL COVER | J | LEVEL SENSORS |
| B | Ø42" CONTAINMENT COLLAR W/ EPOXY SOCKET | K | 4" FIBERGLASS DROP PIPE |
| C | Ø42" CONT. SUMP W/ Ø37" WATERTIGHT TWIST LOCK LID | L | 4" PUMP OUT CONNECTION W/ CAM-LOCK QUICK CONNECT |
| D | 4" HALF COUPLING, NPT MANWAY COVER FITTING | M | 6" FLANGE NOZZLE INLET |
| E | 4" FULL COUPLING, NPT MANWAY COVER FITTING | N | INLET PIPING W/ TEE, CLEAN OUT, AND CAP |
| F | Ø42" H-20 RATED STEEL MANHOLE RING & COVER | O | VENT LINE |
| G | Ø16" H-20 RATED STEEL MANHOLE RING & COVER | P | STEEL LIFTING LUGS |
| H | 4" HALF COUPLING, NPT INTERSTITIAL MONITOR FITTING | Q | ELECTRICAL SPLICE BOX |
| I | LEAK DETECTION SENSOR |  |  |

MFG: 147 Opportunity Rd., Camdenton, MO 65020

DATE:

8/18/2021

Mailing: P.O. BOX 326, Montreal, MO 65591